

EZ4 MINI Manual  
**1）Format the SD card with FAT (EZ4 support 2G SD card)  
2）Please download EZ4 soft and patch ROMs with EZ4 Client.exe. Please patch all of ROMS because compatible of ROMs.**

****

**3）Rename the ROMs in English or numbers which already patched and put them into SD card.  
**

**4）Please run the ROMs on GBA/GBA SP/GBM/NDS.  
EZ4 could direct run the ROM less than 16M on PSRAM but it need a little time of loading for each time.   
Press “A” when you choose a ROM on GBA/GBA SP/GBM/NDS**

**EZ4 could also run the ROM less than 32M on Norflash with burning first.   
Press “SELECT” when you choose a ROM and burn the ROM   
into Norflash first. After 100% burning it should be showed in the EZ-Disk below.**

**5）Kernel update:   
Please download the newest version of EZ4 software and put all of files in the root directory of SD card. Press “R” when you turn on the GBA/GBASP/GBM/NDS. It should be updated after 100% writing.**

**Attention：  
1）PSRAM could run the ROM less than 16M only.**  
**2）Norflash could run the ROM less than 32M but burning first.**

**3）Please patch the ROMs and rename them in English or Numbers with EZ4 Client.exe.**

**Please burn the ROM to Norflash if some ROM could not run on PSRAM.**

**Thank a lot！**

[www.ezflash.cn](http://www.ezflash.cn)

[sales@ezflash.cn](mailto:sales@ezflash.cn)