2011-03-09
Fireware updated to v1.09
1, Fixed: sometimes the cart cannot be recognized after resetting on NDSi/N3DS.
2, Changed: use separate boot program for N3DS/NDSi/NDS.
3, Added: reboot and re-upgrade after Upgrade failed.

2011-03-03
(3DS)DSTWO Fireware ver1.08
Upgrade fireware version with ver1.08, Increase support for N3DS NDS mode for N3DS.
Added a system11.dat file which is a patch file under the _dstwo folder.

How to use:
Copy ds2update.dat file and the newest OS to the root of your microsd card, then insert DSTWO into the DS to upgrade your DSTWO. Make sure DO NOT power off until it finished upgrading! 
Then you can use your DSTWO on the N3DS after upgrading.


2011-03-09
更新固件至1.09
1.修正1.08固件NDSI/3DS 复位重启有时不能识别问题
2.3ds,NDSi,NDS三种主机引导程序分开，相互影响降到最小
3.加入“固件一旦升级失败，能够重新引导升级”的功能

note:


使用方法：拷贝dstwoupdate.dat和最新内核(1.11)到TF卡根目录下，将DSTWO卡插入DS主机后进入DSTWO升级，升级时候 请保证不要断电以及多余的操作！旧固件可以使用新内核，但是不能更新1.09的固件，只有用最新内核（1.11），才能更新最新固件（1.09）。还有就是要正确使用中英版本内核更新对应固件。


2011-3-3
更新固件至1.08，增加支持3DS的NDS模式。
此次还在_dstwo目录增添了system11.dat补丁文件。

使用方法：拷贝ds2update.dat和最新内核到TF卡根目录下，将DSTWO卡插入DS主机后进入DSTWO升级，升级时候 请保证不要断电以及多余的操作！升级完成后就可以在3DS上使用了。

(3DS专用)DSTWO卡带固件升级v1.08（2011-03-04） 
更新固件至1.08，增加支持3DS的NDS模式。
此次还在_dstwo目录增添了system11.dat补丁文件。