           CENTRAL POINT PC TOOLS PRO (VERSION 9)

This file contains information that is not in the manual or has changed
since the manual was printed. Please take a moment to read it.
 
This file is organized into four sections: 
   
   - General Update Information
   - Notes on Specific PC Tools Pro Programs   
   - Miscellaneous Compatibility Notes
   - Notes to System Administrators

=========================================================================

                              
  GENERAL UPDATE INFORMATION
  
  *  When you run Install, configuration files for the
     previous version are stored in the \PCTOOLS\OLDPCT
     directory. For more information on these files and how
     to restore them, see the Installing PC Tools Pro
     chapter in your PC Tools Pro manual.
  
  *  Desktop Accessories and Commute are not included in PC
     Tools Pro. However, if these version 8 applications are
     on your hard disk, they are retained by PC Tools Pro
     Install and continue to launch from PC Tools
     Desktop/Shell. If you delete PC Tools version 8
     programs to free up disk space, you must retain Desktop
     Accessories and Commute files if you want keep using
     these programs. See the PC Tools Files chapter in your
     version 8 manual for a list of applicable files.
  
  *  Data Monitor (DATAMON), now called DPROTECT, takes up
     less memory, and no longer includes Directory Locking,
     Write Protection, or the Screen Blanker. Disk Light is
     now a separate TSR. See the Data Monitor section of
     this file for more information.
  
  *  Compress has been changed to Optimizer (OPTIMIZR) in PC
     Tools Pro. A batch file has been provided to run the
     appropriate program if you type COMPRESS at the command
     line.
  
  *  For the most up-to-date information about new menu
     items, command buttons, and dialog boxes, and about
     features that might work differently than documented in
     the manuals, press F1 in each PC Tools Pro application
     for online help.
  
  *  For a list of command-line options, type /? after the
     program name at the DOS prompt.
  
  NOTES ON SPECIFIC PC TOOLS PRO PROGRAMS
  
  Central Point Anti-Virus
  ------------------------
  
  *  For an explanation of the .INI file settings for Anti-
     Virus, see the CPAV.TXT file in the \PCTOOLS\DATA
     directory. This is an ASCII file and can be viewed or
     printed as needed.
  
  *  When scanning a network server from the command line (using
     /N or /P), you get no visual indicator when the program is
     mapping the directory structure and it may appear locked.
     Since network drives tend to be large, they take longer to
     process.

  *  If you are using the Speedstar 24X Video Board, the
     24XMODE.COM file changes each time it is executed. To
     prevent verification alerts each time the driver is run,
     add this file to your Verification Exceptions list.

  *  When scanning drives that have been compressed with the
     disk-compression utility SuperStor from AddStor, turn
     off the Anti-Stealth option. On such compressed volumes,
     files are compressed and decompressed dynamically, which
     results in their checksums not matching. You may get
     unreliable verification errors.

  Central Point Backup
  --------------------
  
  *  For an up-to-date list of tape drives that Central
     Point Backup supports, see TAPEDRVS.TXT in the
     \PCTOOLS\DATA directory.
  
  *  If you use Central Point Backup version 8.0 backup sets
     with password protection, use the /V8PASS command-line
     option, as follows:
  
      C:\PCTOOLS\CPBACKUP.EXE /V8PASS
  
     If you attempt to use the version 8.0 password-
     protected backup set without this switch, the password
     may not be accepted, even if it is entered correctly.
  
  *  Make sure you close all applications (other than
     CPTASK, Scheduler and Central Point Backup) before
     performing a backup or confidence test. If you do not,
     files that are in use by active applications will not
     be backed up. This could result in compare errors,
     confidence test errors, and, in the case of QIC tape
     drive users, the inability to restore the backup.
  
  *  If you use disk-caching software (such as SMARTDrive or
     PC-Kwik) while performing a medium-speed backup or
     restore, turn off the delayed-write feature of the
     cache program to prevent DMA conflicts. This applies to
     SCSI backups and restores as well. PC-Cache requires no
     changes. These caching programs can often affect
     backups to floppy drives or tape drives connected to
     the floppy controller. Turn off caching of drives A and
     B if you experience problems.
  
  *  Do not back up to a compressed removable disk drive. If
     you do, errors will occur. Instead, use Central Point
     Backup's compression option to back up to a non-
     compressed removable disk drive.
  
  *  Before you use Central Point Backup to back up a
     DoubleSpace drive, run Microsoft's DOUBLESPACE /CHKDSK
     /F to double-check the integrity of the DoubleSpace
     volume.
  
  *  Central Point Backup is set by default to exclude
     hidden and system files from every backup. Therefore,
     if you back up a DoubleSpace, Stacker, SuperStor, or
     other similar compressed drive, Central Point Backup
     does not back up the CVFs (Compressed Volume Files),
     since it is unnecessary to back up these files. If you
     want to back up these files, choose Selection Options
     from the Options menu, and deselect the Hidden
     Attribute and System Attribute options.
  
  *  When using CPS Tape format, incremental backups with
     Data Encryption selected are not supported in this
     version of Central Point Backup.
  
  *  Backup will not find Irwin/Archive 4100C (only applies
     to the 'C' model) tape controllers set to factory-
     default settings. (370-6-2). Try using 360-6-2 or 3E0-6-
     2 by changing the jumper from pin B (for 370) to pin C
     (360) or D (3E0). Almost any setting that does not use
     370 or DMA 2 will work.
  
  *  If you use an Adaptec 1542C controller and are not
     using factory default settings, you might see the
     message "The adapter card could not be configured.
     Initializing and resetting the card did not work." If
     so, run the Adaptec setup program to reset the card to
     the factory default settings, or add this line to your
     CONFIG.SYS file:
  
      DEVICE=C:\PCTOOLS\SYSTEM\ASPI4DOS.SYS
  
     If you have any devices other than a tape drive
     attached to the Adaptec 1542C card, modifying your
     CONFIG.SYS file is the best solution. See the
     ADAPTEC.TXT file in the \PCTOOLS\DATA  directory for
     more information on using Adaptec SCSI cards with
     Central Point Backup.
  
  *  The ~PCACHE file has been added to the list of files
     that Central Point Backup does not back up. Some
     versions of the PCACHE program create files with the
     .$$$ extension that may cause compare or restore
     problems. To avoid this, exclude *.$$$ files in the
     Include/Exclude files list.

  CPR (Central Point Recuperator)
  -------------------------------
  
  *  For more detail about CPR and specific limitations for
     its use with Microsoft Windows and networks, see the
     CPR.TXT file in your \PCTOOLS\SYSTEM directory.
  
  *  CPR Setup cannot install CPR if you are using MS-DOS 6
     Multi-Config in your AUTOEXEC.BAT file. To add CPR to a
     Multi-Config file manually, see your MS-DOS
     documentation.
  
  *  If you have Delete Sentry enabled when you install CPR,
     it might claim there is not enough space on your
     uncompressed drive to save its image file, even though
     DOS reports adequate free space. This is because Delete
     Sentry saves information about deleted file's location,
     but changes the path to the file in the File Allocation
     Table, preventing DOS from finding it.
  
     To make space available, make sure you retrieve any
     deleted files you might want, then purge the deleted
     files in Undelete:
     
       1. From DOS, type Undel and press Enter.
       2. Choose Purge Deleted Files from the File menu.
       3. Select Delete Sentry.
  
  *  Do not load CPRLOW.EXE as a DEVICE HIGH statement
     in your CONFIG.SYS file. This causes your system to
     reboot continuously.

  *  If you are on a network or boot directly to Windows and
     would like CPR to pause each time you boot for optional
     recovery, insert CPR /ASK in your AUTOEXEC.BAT file,
     immediately after the statement that loads your mouse
     or the network IPX, whichever is later in the file. For
     example,
  
      C:\DOS\MOUSE
      C:\NET\IPX
      C:\PCTOOLS\CPR /ASK
      C:\NET\NETX
      C:\WINDOWS\WIN
  
  *  CPR is not compatible with OnTrack Disk Manager, the
     Spectrum/24 graphics card manufactured by SuperMac
     Technology, or Tiga video cards.
  
  *  CPR identifies your computer video type by reading the
     chipset, not by identifying the video board
     manufacturer. For example, you may have a Genoa video
     card that uses a Cirrus 2 chipset. If so, Cirrus 2
     appears in the Advanced Configuration dialog box.
  
  *  New video drivers are being developed continuously for
     CPR and will be made available for downloading from our
     BBS, with an accompanying README file.

  *  If you make changes to your AUTOEXEC.BAT, CONFIG.SYS, or 
     SYSTEM.INI files, you should reinstall CPR. See your manual
     for instructions on reinstallation.
  
  Data Monitor (changed to DPROTECT)
  ----------------------------------
  
  *  Data Monitor (DATAMON) is no longer in PC Tools Pro.
     The Delete Protection functions are now in a smaller
     program called DPROTECT. It is installed using the
     Configure Startup Programs option in PC Config. To
     configure the drives you want to protect, run Undelete
     and choose Configure Delete Protection from the Options
     menu.
  
  *  If you were using other Data Monitor options (such as
     Directory Locking and Write Protection), and want to
     continue using them, do not install DPROTECT.
  
  *  If you were using DATAMON for Disk Light, replace it
     with the PC Tools Pro stand-alone program, Disk Light,
     which performs the same functions as the Disk Light
     feature formerly in Data Monitor. You can install it
     from PC Config's Startup Programs option.
  
  DiskFix
  -------
  
  *  DiskFix recognizes DoubleSpace drives and will diagnose
     and fix problems on the underlying hard disk. Surface
     Scan and Revitalize functions do not operate on
     DoubleSpace drives, but will work on the underlying
     "host" physical drive.
  
  *  DiskFix handles up to 50,000 files and 2,000
     directories if an extended memory manager (such as
     HIMEM.SYS or QEMM.SYS) is installed, and there is
     enough extended memory available. If there is no
     extended memory, DiskFix handles up to 12,000 files and
     1,500 directories.
  
  DriveMap
  --------
  
  *  If you are on a Novell network and map another SPX
     drive using DriveMap from within Windows, the VIPX.386
     Windows network driver might keep DriveMap from working
     properly. To solve this problem, (1) Load DriveMap
     before starting Windows, or (2) edit the Windows
     SYSTEM.INI file to delete VIPX.386 from the NETWORK=
     line. Leave the rest of the line as it is. Although
     most systems are not affected, multiple DOS
     applications can no longer access Novell's IPX services
     simultaneously if you remove this driver.
  
  *  If you are using the parallel port of your AST notebook
     computer with DriveMap, set the parallel port to
     standard mode. To do this, add the following line to
     your AUTOEXEC.BAT file on the AST:
  
      ASTPORT /S
  
  *  The BIOS of some computers, such as Compaqs, might not
     recognize the parallel port of your PC if the cable is
     plugged into it when you turn on the PC. DriveMap
     attempts to resolve this, but if it cannot find the
     parallel port, restart your PC without the cable
     plugged in. Then plug in the cable, and run DriveMap
     again.
  
  Emergency Disk
  --------------
  
  *  The Build Emergency Disk program does not save the
     Iomega DOSLOAD.SYS driver that is used with their
     removable cartridge drives. This is because Iomega uses
     a unique driver technology. You can add any driver to
     your emergency disk manually. Follow the directions for
     adding device drivers to the emergency disk in the
     Build Emergency Disk chapter in the printed manual.
  
  File Check (FILECHK)
  --------------------
  
  *  If you use File Check in a batch file, it returns -253
     when it finds no errors on a DoubleSpace drive. If it
     does find errors, it returns its documented error level
     codes.
  
  Install
  -------
  
  *  The MS-DOS 6 Multi-Config system lets you select how
     your system is configured at boot time. We do not
     recommend this feature for novice or intermediate
     users. If you use Multi-Config, include the PC Tools
     Pro drivers and TSRs you consider essential to all PC
     operations in the "common section" of your
     configuration file.
  
  *  If you are running DR-DOS or a version of MS-DOS
     earlier than 5.0, Install searches your drives for the
     first AUTOEXEC.BAT file in the root directory. If
     Install cannot find the file, it prompts you for the
     location of your AUTOEXEC.BAT file.
  
  *  If you are using Direct Access, the PC Tools Pro
     installation program converts only version 5.1 files
     for use with PC Tools Desktop.
  
  *  Some PC Tools files are in a different directory than
     the one shown in the File List in the printed manual.
     The following files are now in the \PCTOOLS directory:
  
      BALLS.EXE     SKY.IMG     CPSWORLD.FLI
      SKY.EXE       STARS.EXE   COMPRESS.BAT
  
  *  The following file has been added to the PCTOOLS\SYSTEM
     directory, and is the overlay file that handles Stacker
     support for Optimizer:
  
      OPTIMSTK.OVL
  
  *  When you configure Startup Programs during
     installation, batch files executed with a CALL command
     in your AUTOEXEC.BAT file are not run. For example, if
     your AUTOEXEC.BAT file contains a line like CALL
     NET.BAT, which loads your network drivers, PC Tools Pro
     memory-resident programs might not load in the correct
     order because Startup Programs cannot find the network
     drivers. If this is the case, temporarily edit your
     AUTOEXEC.BAT file to load the contents of the batch
     files directly, run PC Config and select the Startup
     Programs you want. Save the configuration, and reboot
     your machine. After you have rebooted, you can edit
     your AUTOEXEC.BAT file to use the CALL command.
  
  Memory Info (MI)
  ----------------
  
  *  If you are using NET5.COM, MI might not identify the
     DOS 5 DOSKey program.
  
  Optimizer (formerly Compress)
  -----------------------------
  
  *  To ensure data integrity, Optimizer does not attempt to
     operate on network and SUBST drives, CD-ROMs, and
     drives accessible through DriveMap.
  
  *  In case of a power failure that results in lost
     clusters or cross-linked files on a DoubleSpace or
     Stacker volume, run DBLSPACE CHKDSK /F or for Stacker
     use CHECK /F or SCHECK /F and answer NO when asked if
     you want to convert a cluster chain into a file. Then
     use DiskFix to verify the integrity of the DoubleSpace
     or Stacker volume.
  
  PC-Cache
  --------
  
  *  DoubleSpace, Stacker, and SuperStor drives default to
     read-only caching when PC-Cache loads. Do not activate
     write-caching for these drives from the user interface
     or the command line.
  
  PC Format
  ---------
  
  *  If you run PCFORM /S from any drive on a DoubleSpace
     system, to create a bootable floppy, for example, PC
     Format might return an error stating that system files
     cannot be found. This problem occurs if the DoubleSpace
     driver has fixed a corrupted boot sector when it is
     rebooted. Unfortunately, the DoubleSpace driver does
     not replace the normal signature of the entire boot
     record.
  
  *  To prevent such boot sector problems on a DoubleSpace
     drive, run BootSafe. BootSafe detects the changed boot
     record signature and alerts you. You can then select
     Rebuild to repair the boot record completely.
  
  *  Note that you cannot format a DoubleSpace drive with PC
     Format.
  
  PC Tools Desktop/Shell
  ----------------------
  
  *  The Reset Window Size command in the Windows menu
     allows you to reset all PC Tools Desktop windows to
     their default sizes and locations. If you change the
     video mode from large to small (such as from 50-line to
     25-line), the open windows are reset to their default
     size and position if any single window cannot fit on
     the smaller screen. If you change the video mode from
     small to large, such as 25-line or 50-line, the open
     windows remain in their current position.
  
  *  If you are not using delete protection (either Delete
     Tracker or Delete Sentry), the Undelete command is not
     available in the Tools menu. To install delete
     protection, choose Configure Startup Programs in PC
     Config, and then select Delete Protection. To configure
     delete protection, run Undelete and choose Configure
     Delete Protection from the Options menu.
  
  RAMBoost
  --------
  
  *  For an explanation of the .INI file settings, and
     information about using RAMBoost with MS-DOS 6 Multi-
     Config, see the RAMBOOST.TXT file in your \PCTOOLS\DATA
     directory.
  
  *  Use PC Config's Startup Programs option to load
     RAMBoost, especially if the RAMBoost directory is not
     in your path.
  
  *  RAMBoost supports PC-DOS, MS-DOS versions 3.3 though
     6.2, DR-DOS version 6.0, and Novell DOS version 7.
  
  *  RAMBoost can be installed on a Stacker 3.1 drive or in
     a MS-DOS 6 environment only if the entire drive is
     compressed. If you install PC Tools Pro on a compressed
     logical drive partition, RAMBoost is installed in a
     \RAMBOOST subdirectory of the root directory of the
     master partition on the drive.
  
    For example, if you install PC Tools Pro on a
     compressed logical drive E on your C hard drive,
     RAMBoost is installed in C:\RAMBOOST. To run RAMSETUP
     or RAMBoost with command-line options, either type the
     full path name, or add C:\RAMBOOST to the PATH
     statement in your AUTOEXEC.BAT file.
  
  *  To avoid redundancy and potential conflicts, do not use
     RAMBoost and Microsoft MemMaker together. RAMBoost
     provides all of the features of MemMaker and has the
     advantage of automatically detecting and adjusting to
     changes in your system configuration, as, for example,
     when you install new software. MemMaker, on the other
     hand, must be run manually after each change to your
     system to ensure optimum use of high memory. If you are
     using RAMBoost and want to experiment with MemMaker,
     first uninstall RAMBoost from your system by running PC
     Config.
  
  *  RAMBoost works in conjunction with your memory manager
     to make the best use of your memory. If you use
     RAMBoost, do not use your memory manager's optimization
     program because RAMBoost replaces that functionality.
     If you have used the other memory optimization program
     already, run RAMSETUP. RAMSETUP removes the previous
     LOAD HIGH syntax and restarts the system.
  
  *  If RAMBoost halts in Learn mode and you are using a
     SCSI device such as ASPI4DOS.SYS, relocate the device
     driver at the beginning of your CONFIG.SYS file. It
     MUST be executed before HIMEM.SYS.
  
  *  If you are using RAMBoost, Windows, and QEMM 6.0, and
     encounter QEMM errors, upgrade to QEMM version 6.02 or
     later.
  
  *  RAMBoost does not strip LH and similar commands from
     nested batch files that are called by your AUTOEXEC.BAT
     file. To ensure that RAMBoost optimizes all memory-
     resident programs, remove the LH and similar commands
     from all called batch files.
  
  *  If you are using a Token Ring adapter, make sure your
     Token Ring drivers are loaded BEFORE PC Tools RAMSETUP
     runs. This allows RAMSETUP to properly protect the
     Token Ring memory addresses.
  
  *  Certain TSRs and device drivers might not get loaded
     high because of an unusually large initialization size.
     You can edit your RAMBOOST.INI file to instruct
     RAMBoost to try other optimization methods. We
     recommend that you use the optmethod option with a -1
     value. See the RAMBOOST.TXT file for instructions.
  
  System Information Pro
  ----------------------
  
  *  Some older 286-class and 386-class computers might
     exhibit problems with the motherboard tests. Some of
     these computers use non-standard chipsets and non-
     standard BIOS. Most newer machines conform to a
     standard architecture.
  
  *  If you use a display adapter that has VESA extensions
     in the on-board BIOS along with a memory-manager, boot
     your computer with your emergency disk when performing
     the Super VGA and Color bar tests. The memory manager
     tries to use the same memory addresses as the VESA, and
     although SI Pro might find the VESA extensions, it
     might perform the tests incorrectly.
  
  *  Super VGA tests may fail on some Trident 8900C 1MB
     video boards. This is because the video chipset reports
     that a HI-Color DAC (digital to analog converter) is
     present when, in fact, the DAC is not capable of
     supporting Hi-Color.
  
  *  Some older BIOS might not show more than two serial
     ports (COM 1 and COM 2), even though a third or fourth
     might exist. SI Pro reports only ports that are seen by
     the BIOS.
  
  *  The PCM sound test might sound unclear if you run SI
     Pro from a floppy disk. This is caused by DMA channel
     conflicts.
  
  Task Switcher
  -------------
  
  *  Scheduling functions are now being handled by Task
     Switcher. If you have a previous version of CPSCHED
     loaded in memory, remove it and use CPTASK.
  
  *  For an explanation of the Task Switcher .INI settings,
     see CPTASK.TXT in your PCTOOLS\DATA directory.
  
  *  Some PC Tools Pro applications provide only limited
     access to Task Switcher to make sure your data stays
     intact during low-level disk access. You cannot use the
     hot key to open Task Switcher from within the following
     applications:
  
      FileFix      Optimizer         Wipe
      Undelete     Unformat          PC Format
      DiskFix (while fixing or checking a disk) CP Backup
  
  *  Similarly, while Task Switcher is open and at least one
     other application is in the Task Switcher list, you
     cannot switch to Optimizer or Undelete. If you switch
     to DiskFix in this situation, you are notified of disk
     errors, but cannot fix them. To repair errors, you must
     end all tasks, and restart DiskFix.
  
  *  Do not use a batch file to unload Task Switcher. If you
     do so, commands following the CPTASK /U command are not
     executed. Do not delete the primary DOS prompt from the
     Task Switcher list if you are using NDOS or 4DOS. Task
     Switcher can be unloaded only from the primary prompt.
  
  *  You can use the Idle Task function in Task Switcher as
     a pseudo screen blanker. Specify any of the following
     screen-blanker files in the \PCTOOLS directory as the
     Idle Task:
  
      BALLS.EXE, SKY.EXE, STARS.EXE, CPSWORLD.FLI
  
     However, unlike most screen blankers, the Idle Task
     function does not auto-cancel (detect keyboard/mouse
     activity and then return to the prior task).
  
     In addition, included in the PC Tools Pro package is a
     program called FLIPLAY.EXE that you can use to run
     animation files as screen blankers. To see an example,
     from the PCTOOLS directory type:
  
      FLIPLAY CPSWORLD.FLI
  
  *  If you have Task Switcher configured to load
     automatically at start up from your AUTOEXEC.BAT file
     and QEMM 7.1's Optimize program adds the LOADHI
     statement to CPTASK, do not unload Task Switcher using
     CPTASK /U or from the main window. Either edit your
     AUTOEXEC.BAT file to remove the LOADHI statement or
     remove CPTASK before running Optimize.
  
  VSafe\VWatch
  ------------
  *  Some problems have been detected when loading VSafe and
     using the SQUEEZE option in QEMM or the FLEXFRAME option
     in 386MAX. For best results, do not use either of these
     options if you are loading VSafe.
  
  *  If you get the message "386MAX VxD error V1014: Disk Cache
     or other file IO software using EMS memory" when using
     VSafe with 386MAX, load VSafe using the /NE option.
  
  *  VSafe does not display a warning when you are running a DOS
     program in graphics mode (such as DESQview); instead, an
     alarm sounds and the action stops. Exit from the program
     and run Central Point Anti-Virus to verify the integrity of
     files.
  
  *  If you want to use both VSafe and KEYB.COM, load VSafe
     after loading KEYB.COM.

  MISCELLANEOUS COMPATIBILITY NOTES
  
  Compaticard Users
  -----------------
  
  *  Compaticards with 2.88MB floppy drives attached are
     incompatible with PC Tools Pro applications.
  
  DESQview Users
  --------------
  
  *  For optimum performance with DESQview, PC Tools Pro
     applications disable the alternate graphic fonts and
     the graphics mouse cursor.
  
  *  If your video display blinks when you use DESQview with
     PC Tools Pro applications, add the Palette utility to
     the DESQview menu and turn off the Blink Enable option.
     For the best display when you run PC Tools Pro
     applications from DESQview, select DESQview in the PC
     Config color scheme list.
  
  DOS APPEND Users
  ----------------
  
  *  The DOS APPEND program has no effect while most PC
     Tools Pro applications are running.
  
  LaserTools PrintCache Users
  ---------------------------
  
  *  If the LaserTools PrintCache program is resident while 
     performing a backup, the backup or a subsequent restore
     might fail. Central Point strongly recommends that you 
     unload PrintCache before running a backup. For details
     on unloading PrintCache, see Chapter 3 of the PrintCache
     manual.
  
  Logitech Mouse Users
  --------------------
  
  *  The Logitech's mouse driver version 4.10 has known
     compatibility problems with DOS 4.0 or later. Upgrade
     to the newest mouse driver, version 6.12 or later.
  
  Infoselect Users
  ----------------
  
  *  If you are using Infoselect 2.0, be sure it is loaded
     before PC Tools Desktop in your AUTOEXEC.BAT file.
  
  MS-DOS 6 DoubleSpace Users
  --------------------------
  
  *  Other than DiskFix and Optimizer, PC Tools Pro
     applications might report a drive size for a
     DoubleSpace drive that is larger than the size reported
     by Microsoft's CHKDSK program. CHKDSK makes estimates
     based on known compression statistics. If there are
     differences, the CHKDSK estimate is probably more
     accurate.
  
  *  See other DoubleSpace notes in the PC Tools program
     notes above.
  
  Packard Bell Mouse Users
  ------------------------
  
  *  The Packard Bell mouse driver version 4.0 is not fully
     compatible with PC Tools Pro. Use the Microsoft Mouse
     driver version 6.14 or later instead. (A recent
     Microsoft mouse driver is usually included with Windows
     or DOS.)
  
  REALTEK VGA Video Card Users
  ----------------------------
  
  *  REALTEK VGA video cards may cause distorted a screen
     display in PC Tools Pro applications. The distortion is
     caused by the graphic mouse. To remedy this, choose
     Mouse Options in PC Config and deselect the graphics
     mouse cursor.
  
  SuperStor Users
  ---------------
  
  *  SuperStor uses a non-standard boot record, which might
     prevent PC Format and the Build Emergency Disk program
     from finding the system files needed to create a
     bootable system disk. Run PC Format and the Build
     Emergency Disk program from the original boot drive
     (the one CONFIG.SYS is on).
  
     Example: D:EDISK /BOOT_DEV=x: (where x=original
     boot drive)
  
  SYSGEN Users
  ------------
  
  *  PC Tools Pro supports the SYSGEN bridge driver versions
     3.44 and above.
  
  Tandy Users
  -----------
  
  *  PC Tools Pro includes the FIXTANDY.EXE program. If you
     have a Tandy system, and the Tandy Setup program
     sometimes runs unexpectedly, make sure FIXTANDY is
     memory-resident before you use any PC Tools Pro
     application. To do so, add C:\PCTOOLS\FIXTANDY to your
     AUTOEXEC.BAT file.
  
  Toshiba 5100 Laptop Users
  -------------------------
  
  *  If some characters do not appear as expected when you
     run PC Tools Pro applications, run PC Config. Select
     Display, Text Mode, and choose OK. Then select Color,
     and choose the Toshiba Gas Plasma color scheme. Choose
     Save, then reboot the machine so that the changes will
     take effect.
  
  UltraVision Users
  -----------------
  
  *  PC Tools Pro applications work with UltraVision fonts,
     but disable the Central Point alternative "graphic"
     font set.
  
  *  If your mouse does not function normally when you use
     non-standard line modes (modes other than 80x25, 80x28,
     80x43, 80x50), disable the Fast Mouse Reset option in
     PC Config, or use the /PS2 command-line option when
     starting a PC Tools Pro application.
  
  NOTES TO SYSTEM ADMINISTRATORS
  
  VSafe/VWatch
  ------------
  
  *  The ISCPSTSR.EXE program that Central Point Anti-Virus
     uses to check the system for resident protection can now
     check to see if users are running a specific version 2.x
     TSR. If you specify VSafe on the command-line, and users
     are running VSafe Version 1.4, ISCPSTSR returns an error
     level indicating that VSafe is not running. It will only
     recognize VSafe and VWatch Version 2.x.
  
     To specify that users accessing the network use VSafe or
     VWatch, use the following format in the system LOGIN
     script:
  
       #ISCPSTSR VSAFE
       or
       #ISCPSTSR VWATCH
  
     If you want ISCPSTSR to check for earlier versions of
     VSafe or VWatch, use the ISCPSTSR command without
     specifying VSAFE or VWATCH. For more information on using
     ISCPSTSR.EXE, see the PC Tools Pro in a Network Environment
     chapter in the manual.
  
  CInstall
  --------
  *  If you are making a set of customized installation
     disks and want to configure them so that users install
     both RAMBoost and CPR, only RAMBoost is configured when
     a user installs. Both RAMBoost and CPR must reboot the
     system before installing, so it is not possible to
     automatically configure both. Users need to be
     instructed to install and configure CPR manually by
     choosing CPR from the Configure Startup Programs option
     in PC Config. See the CPR chapter in the manual for
     additional instructions.
